
Time Baby V13 Configuration File Memory Map

This image describes some of the settings defined in the file "CONFIG.TB" used by Time Baby.
Not all of these settings can be adjusted through the program interface, so there is some
potential for a seperate configurator program that could be written to adjust these settings.
If no such program is ever written, the configuration file can easily be modified with any
hex editor program such as Breakpoint Hex Workshop.

The last four bytes in the config file are considered set if their value is changed to anything
other than zero, and not set if their value is zero. The option to deactivate the infrared port
was included because the port may consume a little extra power, but I haven't tested to be sure
this is true. The infrared port is active when it's config byte is set to zero.

There are many other locations in use by the program that are not explained here, but they can
all be set through the program interface as explained in the program documentation.

Cheers, Art.
